**Build ‘em up! Break ‘em down! By: Devin Humphrey**

“Step by Step Guide to Mowing a Yard”

Step 1: Evaluate the surrounding are for rocks, stumps, or any type of obstacles that could render your mowing capabilities.

Step 2: Clear and mark obstacles for a refined scope of the yard to be mowed.

Step 3: Ensure your mower has clean oil by locating and checking the level, predetermined by the mower manufacturer.

Step 4: If you do not know the predetermined oil level, contact the manufacture or online reference for guidance.

Step 5: If the mower is low on oil fill to desired level.

Step 6: Ensure the mower has the appropriate fuel, determined by the manufacture.

Step 7: If the mower doesn’t have the desired full or meet the level to operate, fill it up.

Step 8: Ensure the mower is clear of obstructions and safe to operate by physically checking the deck, pinch points, tire pressure, blades, and engine compartment.

Step 9: Locate and insert the proper key for the mower, determined by the manufacture.

Step 10: Adjust the cutting dept of the mower to the appropriate and desirable level.

Step 11: Ensure you wear safety approved eyeglasses, earplugs, and gloves for protection against foreign material and excessive noise.

Step 12: Ensure the choke is engaged determined by the manufacture.

Step 13: Start the mower and readjust the choke to the normal operating condition.

Step 14: If the mower doesn’t start contact a repair facility near you

Step 15: If the mower starts, conduct another visual to ensure no children are present around your vicinity.

Step 16: Engage the deck by pressing or manipulating a lever determined by the manufacture.

Step 17: Determine the desired mowing pattern for best results.

Step 18: Press the throttle determined by the manufacture. Happy Mowing!